**Glass fabric 25 g/m²**

**Finish FRP 800 (Interglas 02034)**

**Application:**  
Wood facing/woodgrain foil (wing linings), honeycomb sandwich components (min 2 layers), PCBs

**Calculated data for hand laminates with 35 volume percent** **fibres:**  
Resin consumption: 20 g/m², laminate thickness: 0,027 mm, laminate weight: 45 g/m²